IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2020-11-10T17:04:24"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1605027865 (2020-11-10T17:04:25Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1605027865 (2020-11-10T17:04:25Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" | FLOOR | names: "NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" | material: layers "NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" ("NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" 1.2) | property sets: COBie

Types
  IFCSLABTYPE "NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" | FLOOR | 1 occurrence | material: layers "NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" ("NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" 1.2) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_08_08:Bitumen sheets" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Bituminous gas and water proof sheet" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Sustainable and innovative multi-function barrier membrane with industry leading performance" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@juta.co.uk" (IFCTEXT)
    Material = "Bitumen and LDPE" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "JUTA GP SAM" (IFCTEXT)
    Name = "BitumenSheets_JUTAGPSAM_JutaUKLtd" (IFCTEXT)
    NominalHeight = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 20000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Flat sheet applied - supplied in roll form" (IFCTEXT)
    Size = "20000 x 900 x 1.2 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "60 Years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Smooth" (IFCTEXT)
    FireRating = "to EN 13501: Euro Class F" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_JutaUKLtd_BitumenSheets_JUTAGPSAM" (IFCTEXT)
    ManufacturerName = "Juta UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.juta.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/tlkgdmnh" (IFCTEXT)
    NBSDescription = "Bitumen sheets" (IFCTEXT)
    NBSReference = "45-65-50/304" (IFCTEXT)
    ProductInformation = "https://www.juta.co.uk/gas-protection-membranes/ground-gas-membranes/gpg1-titansam/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_08_08" (IFCTEXT)
    Uniclass2015Title = "Bitumen sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    FirePerformance = "to EN 13501: Euro Class F" (IFCTEXT)
    Form = "Bitumonous gas and water proof sheet" (IFCTEXT)
    MaterialBitumenModification = "n/a" (IFCTEXT)
    MaterialCarrierMaterial = "n/a" (IFCTEXT)
    MaterialGasInhibitor = "Aluminium foil" (IFCTEXT)
    MaterialRootInhibitor = "n/a" (IFCTEXT)
    MembraneCarrierMaterial = "n/a" (IFCTEXT)
    Standard = "BS 8485:2015, BS8102:2009, CIRIA C735" (IFCTEXT)
    SurfaceFinishesTop = "White cross laminated high-density polyethylene" (IFCTEXT)
    SurfaceFinishesUnderside = "Siliconized paper release film" (IFCTEXT)
    ThicknessMinimum = "1 mm" (IFCTEXT)
    ThirdPartyProductCertification = "CE certified: EN 13967:2012 + A1:2017" (IFCTEXT)
    Weight = "1100 g/m²" (IFCTEXT)
    WidthOptions = "300 mm, 900 mm" (IFCTEXT)