IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2020-11-10T17:04:25"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1605027866 (2020-11-10T17:04:26Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1605027866 (2020-11-10T17:04:26Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" | FLOOR | names: "NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" | material: layers "NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" ("NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" 0.8) | property sets: COBie

Types
  IFCSLABTYPE "NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" | FLOOR | 1 occurrence | material: layers "NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" ("NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" 0.8) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_65_60:Plastics sheets" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Multi-layer, polythylene membrane with polythyrene reinforcing grid" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "High Performance BBA Certified Radon Barrier DPM" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@juta.co.uk" (IFCTEXT)
    Material = "Polythylene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "JUTA GP4" (IFCTEXT)
    Name = "PlasticsSheets_JUTAGP4_JutaUKLtd" (IFCTEXT)
    NominalHeight = 0.6 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 50000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Flat sheet applied - supplied in roll form" (IFCTEXT)
    Size = "2000 x 50000 x 0.6 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Minimum 60 Years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_JutaUKLtd_PlasticsSheets_JUTAGP4" (IFCTEXT)
    ManufacturerName = "Juta UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.juta.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/3p1vu5zv" (IFCTEXT)
    NBSDescription = "Plastics sheets" (IFCTEXT)
    NBSReference = "45-65-50/325" (IFCTEXT)
    ProductInformation = "https://www.juta.co.uk/gas-protection-membranes/radon-membranes/juta-gp4/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_65_60" (IFCTEXT)
    Uniclass2015Title = "Plastics sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Form = "Low density polythylene membrane with reinforcing grid" (IFCTEXT)
    PerformanceAntistaticProperties = "n/a" (IFCTEXT)
    PerformanceColour = "Beige" (IFCTEXT)
    PerformanceElongationToBreak = "0.15" (IFCTEXT)
    PerformanceFirePerformance = "n/a" (IFCTEXT)
    PerformanceResistantToUndergroundGases = "Radon - 1.7 x 10(-11)" (IFCTEXT)
    PerformanceTearResistance = "500 N" (IFCTEXT)
    PerformanceTensileStrengthMinimum = "570 N/50 mm" (IFCTEXT)
    PerformanceUvStabilization = "n/a" (IFCTEXT)
    PerformanceWaterVapourResistanceMinimum = "n/a" (IFCTEXT)
    PhysicalPropertiesDimensionsRollLengthMinimum = "50 m" (IFCTEXT)
    PhysicalPropertiesDimensionsThicknessMinimum = "0.6 mm" (IFCTEXT)
    PhysicalPropertiesDimensionsWidthMinimum = "2 m" (IFCTEXT)
    PhysicalPropertiesWeightMinimum = "400 G/ M2" (IFCTEXT)
    Purpose = "Radon, air and moisture protection system" (IFCTEXT)
    RecycledContent = "0" (IFCTEXT)
    RootInhibitor = "n/a" (IFCTEXT)
    Standard = "BR211-2015" (IFCTEXT)
    ThirdPartyCertification = "CE Mark - EN13967:2012, BBA Certified - Certificate No. 20/5728 (P5)" (IFCTEXT)