IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2020-11-10T17:04:25"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1605027866 (2020-11-10T17:04:26Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1605027866 (2020-11-10T17:04:26Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" | FLOOR | names: "NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" | material: layers "NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" ("NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" 8.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" | FLOOR | 1 occurrence | material: layers "NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" ("NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" 8.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_15_57_27_39:Geosynthetic clay liners (GCLs)" (IFCTEXT)
    CodePerformance = "BS 8102: 2009" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Mechanically bonded Geosynthetic Clay linear" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Pre-Applied Self Healing Waterproofing Membrane" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@juta.co.uk" (IFCTEXT)
    Material = "Pulverised Bentonite & Geotextile" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "JUTA Hydrolock" (IFCTEXT)
    Name = "GeosyntheticClayLiners_JUTAHydrolock_JutaUKLtd" (IFCTEXT)
    NominalHeight = 8. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 5100. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1250. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Supplied in roll form" (IFCTEXT)
    Size = "1250 x 5100 x >7 mm" (IFCTEXT)
    SustainabilityPerformance = "Consult manufacturer" (IFCTEXT)
    WarrantyDescription = "60 Year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_JutaUKLtd_GeosyntheticClayLiners_JUTAHydrolock" (IFCTEXT)
    ManufacturerName = "Juta UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.juta.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/jgikznkn" (IFCTEXT)
    NBSDescription = "Geosynthetic clay liners (GCLs)" (IFCTEXT)
    NBSReference = "45-65-35/345" (IFCTEXT)
    ProductInformation = "https://www.juta.co.uk/waterproofing/type-a/hydrolock/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_15_57_27_39" (IFCTEXT)
    Uniclass2015Title = "Geosynthetic clay liners (GCLs)" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    IntegralAccessories = "Hyrdolock strip, Hydrolock Paste, Hydrolock Rail" (IFCTEXT)
    ThirdPartyProductCertification = "BBA Certificate 18/5547" (IFCTEXT)
    Weight = "5300 g/m²" (IFCTEXT)