IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2020-11-10T17:04:25"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1605027865 (2020-11-10T17:04:25Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1605027865 (2020-11-10T17:04:25Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" | FLOOR | names: "NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" | material: layers "NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" ("NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" 0.8) | property sets: COBie

Types
  IFCSLABTYPE "NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" | FLOOR | 1 occurrence | material: layers "NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" ("NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" 0.8) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_65_60:Plastics sheets" (IFCTEXT)
    CodePerformance = "BS 8485:2015 + A1 2019 Accordant" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Multi-layer, low density polythylene membrane" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 Years" (IFCTEXT)
    Features = "Multi-layer, low density polythylene membrane" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@juta.co.uk" (IFCTEXT)
    Material = "Polypropylene and Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "JUTA GP1" (IFCTEXT)
    Name = "PlasticsSheets_JUTAGP1_JutaUKLtd" (IFCTEXT)
    NominalHeight = 0.6 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 50000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Flat sheet applied - supplied in roll form" (IFCTEXT)
    Size = "50000 x 2000 x 0.6 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Minimum 60 Years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_JutaUKLtd_PlasticsSheets_JUTAGP1" (IFCTEXT)
    ManufacturerName = "Juta UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.juta.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/2xss2rdm" (IFCTEXT)
    NBSDescription = "Plastics sheets" (IFCTEXT)
    NBSReference = "45-65-50/325" (IFCTEXT)
    ProductInformation = "https://www.juta.co.uk/gas-protection-membranes/ground-gas-membranes/gp1/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_65_60" (IFCTEXT)
    Uniclass2015Title = "Plastics sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Form = "Polypropylene reinforcing grid with aluminium foil" (IFCTEXT)
    PerformanceAntistaticProperties = "n/a" (IFCTEXT)
    PerformanceColour = "Black" (IFCTEXT)
    PerformanceElongationToBreak = "0.2" (IFCTEXT)
    PerformanceFirePerformance = "n/a" (IFCTEXT)
    PerformanceResistantToUndergroundGases = "Methane - 0.09 ml/m²/day atm. Carbon Dioxide - 0.09 ml/m²/day/atm. Radon - 8 x 10(-15)" (IFCTEXT)
    PerformanceTearResistance = "330 N, 400 N" (IFCTEXT)
    PerformanceTensileStrengthMinimum = "480 N/50 mm" (IFCTEXT)
    PerformanceUvStabilization = "n/a" (IFCTEXT)
    PerformanceWaterVapourResistanceMinimum = "n/a" (IFCTEXT)
    PhysicalPropertiesDimensionsRollLengthMinimum = "50 m" (IFCTEXT)
    PhysicalPropertiesDimensionsThicknessMinimum = "0.6 mm" (IFCTEXT)
    PhysicalPropertiesDimensionsWidthMinimum = "2 m" (IFCTEXT)
    PhysicalPropertiesWeightMinimum = "370 G/ M²" (IFCTEXT)
    Purpose = "Gas-resistant barrier to restrict the ingress of radon, methane and carbon dioxide into buildings from landfill and naturally occurring sources" (IFCTEXT)
    RecycledContent = "0" (IFCTEXT)
    RootInhibitor = "n/a" (IFCTEXT)
    Standard = "BS 8485:2015 + A1 2019 Accordant" (IFCTEXT)
    ThirdPartyCertification = "BBA Certified - Certificate No. 12/4912, CE Mark - EN13967:2012" (IFCTEXT)